IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-11-20T09:57:41"
Originating system: "SketchUp Pro 2015"
Application: "SketchUp Pro 2015" version "2015" identifier "2015" by Organization "SketchUp"

People and organizations
  Person (no name given) of Organization "SketchUp"
  Owner history of Person (no name given) of Organization "SketchUp" | application "SketchUp Pro 2015" version "2015" identifier "2015" by Organization "SketchUp" | change ADDED | created 1732093061 (2024-11-20T08:57:41Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Default Project" | description "Description of Default Project"
  IFCSITE "Default Site" | latitude 24° 28′ 0″ | longitude 54° 25′ 0″ | elevation above sea level 10. | description "Description of Default Site"
    IFCBUILDING "Default Building" | postal address (none given) | description "Description of Default Building"
      IFCBUILDINGSTOREY "Default Building Storey" | elevation 0. | description "Description of Default Building Storey"
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | descriptions: "Description of Object"
      IFCBUILDINGSTOREY "Default Building Storey" | elevation 0. | description "Description of Default Building Storey"
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | names: "慈摮搠祲牥䤠敢潲㈠〲㈭〴⁖〵㘯䠰z" | descriptions: "Description of Object" | property sets: SU_InstanceSet, SU_DefinitionSet, CompositionType, Name, CalculatedGeometryValues, OrientedBoundingBox

Property sets
  SU_InstanceSet | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Owner = "" (IFCLABEL)
    Status = "" (IFCLABEL)
  SU_DefinitionSet | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Price = "" (IFCLABEL)
    Size = "" (IFCLABEL)
    Url = "" (IFCLABEL)
  CompositionType | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IfcElementCompositionEnum = "complex" (IFCLABEL)
  Name | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IfcLabel = "Hand dryer Ibero 220-240V 50/60Hz" (IFCLABEL)
  CalculatedGeometryValues | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 2.883E-1 (IFCREAL)
    CenterOfGravityX = -1.43677 (IFCREAL)
    CenterOfGravityY = -80.7086 (IFCREAL)
    CenterOfGravityZ = 105.873 (IFCREAL)
    IsSolid = TRUE (IFCBOOLEAN)
    Volume = 9.688810000000001E-3 (IFCREAL)
  OrientedBoundingBox | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Name = "Hand dryer Ibero 220-240V 50/60Hz" (IFCLABEL)
    OX = -3.78457E-1 (IFCREAL)
    OY = -67.931 (IFCREAL)
    OZ = 112.288 (IFCREAL)
    XX = -3.72896 (IFCREAL)
    XY = 100.613 (IFCREAL)
    XZ = -38.1378 (IFCREAL)
    YX = -31.4463 (IFCREAL)
    YY = 50.4908 (IFCREAL)
    YZ = 136.276 (IFCREAL)
    ZX = 157.698 (IFCREAL)
    ZY = 17.2199 (IFCREAL)
    ZZ = 30.0093 (IFCREAL)
  ePset_BIMobjectScript | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Colour = "AA92000 - Polished Stainless Steel" (IFCLABEL)
    LOD = "300" (IFCLABEL)
  ePset_BIMobject_BO | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    BO_classific = "" (IFCLABEL)
    BO_links = "" (IFCLABEL)
    BO_real = "" (IFCLABEL)
    BO_regions = "" (IFCLABEL)
    BimObjectCategory (BO_bocat) = "Dryers (Hand & Hair)" (IFCLABEL)
    BimObjectCategoryCode (BO_bocat_code) = "sanitary-hand-and-hair-dryers" (IFCLABEL)
    BimObjectMainCategory (BO_bomaincat) = "Sanitary" (IFCLABEL)
    BimObjectMainCategoryCode (BO_bomaincat_code) = "sanitary" (IFCLABEL)
    BrandUrl (BO_brandurl) = "http://jofel.com" (IFCLABEL)
    COBIeTypeCategory (BO_cobie_type_cat) = "" (IFCLABEL)
    Depth (BO_depth) = 210. (IFCREAL)
    DesignCountry (BO_designcont) = "Spain" (IFCLABEL)
    EditionNumber (BO_edinum) = "" (IFCLABEL)
    GtinCode (BO_gtin) = "" (IFCLABEL)
    Height (BO_height) = 220. (IFCREAL)
    IfcClassification (BO_ifcclas) = "Electric Appliance" (IFCLABEL)
    InstallationInstructions (BO_montins) = "" (IFCLABEL)
    InstructionVideo (BO_youtube) = "https://jofel.com/media/fichas/en/AA92000.pdf" (IFCLABEL)
    ManufacturCountry (BO_mancont) = "Spain" (IFCLABEL)
    ManufacturName (BO_Manufac) = "Jofel" (IFCLABEL)
    MasterFormat2014Code (BO_masterformat2014_code) = "10 28 13" (IFCLABEL)
    MasterFormat2014Description (BO_masterformat2014_name) = "Toilet Accessories" (IFCLABEL)
    MaterialMain (BO_mainmat) = "Stainless steel" (IFCLABEL)
    MaterialSecondary (BO_secmat) = "ABS" (IFCLABEL)
    NBSReference (BO_nbs_ref) = "02-03" (IFCLABEL)
    NBSReferenceDescription (BO_nbs_desc) = "Air Dryers" (IFCLABEL)
    OmniClassCode (BO_omniclass_code) = "23-31 25 15" (IFCLABEL)
    OmniClassDescription (BO_omniclass_name) = "Hand Dryers" (IFCLABEL)
    ProductCertification (BO_prodcert) = "" (IFCLABEL)
    ProductDataUrl (BO_prodaturl) = "bimobject.com/jofel/product/hand_dryer_ibero_inox_220-240V_50-60hz" (IFCLABEL)
    ProductFamily (BO_prodfam) = "Hand dryers" (IFCLABEL)
    ProductGroup (BO_prodgroup) = "Ibero" (IFCLABEL)
    ProductGuid (BO_productguid) = "17c93de5-44ca-4e0a-8acd-4e8b2e910c59" (IFCLABEL)
    ProductName (BO_prodinfo) = "Hand dryer Ibero 220-240V 50/60Hz" (IFCLABEL)
    ProductUrl (BO_producturl) = "https://jofel.com/en/productos/secadores-de-mano/secamanos-ibero-brillo-optico.html" (IFCLABEL)
    PublishDate (BO_publisdat) = "" (IFCLABEL)
    QR (BO_boqrurl) = "http://bimobject.com/jofel/product/hand_dryer_ibero_inox_220-240V_50-60hz" (IFCLABEL)
    RegionAfrica (BO_africa) = "AO, BF, BI, BJ, BW, CD, CF, CG, CI, CM, CV, DJ, DZ, EH, ER, ET, GA, GH, GM, GN, GQ, GW, KE, KM, LR, LS, LY, MA, MG, ML, MR, MU, MW, MZ, NA, NE, NG, RE, RW, SC, SD, SH, SL, SN, SO, SS, ST, SZ, TD, TG, TN, TZ, UG, YT, ZA, ZM, ZW" (IFCLABEL)
    RegionAntarctica (BO_antarctica) = "None" (IFCLABEL)
    RegionAsia (BO_asia) = "AM, AZ, BD, BN, BT, CC, CN, CX, GE, HK, ID, IN, IO, JP, KG, KH, KP, KR, KZ, LA, LK, MM, MN, MO, MV, MY, NP, PH, PK, SG, TH, TJ, TM, TW, UZ, VN" (IFCLABEL)
    RegionEurope (BO_europe) = "AD, AL, AT, AX, BA, BE, BG, BY, CH, CY, CZ, DE, DK, EE, ES, FI, FO, FR, GB, GG, GI, GR, HR, HU, IE, IM, IS, IT, JE, LI, LT, LU, LV, MC, MD, ME, MK, MT, NL, NO, PL, PT, RO, RS, RU, SE, SI, SK, SM, UA, VA" (IFCLABEL)
    RegionMiddleEast (BO_middleeast) = "AE, BH, EG, IL, IQ, IR, JO, KW, LB, OM, PS, QA, SA, TR, YE" (IFCLABEL)
    RegionNorthAmerica (BO_northamerica) = "AG, AI, AW, BB, BL, BM, BQ, BS, BZ, CA, CR, CU, CW, DM, DO, GD, GP, GT, HN, HT, JM, KN, KY, LC, MF, MQ, MS, MX, NI, PA, PM, PR, SV, SX, TC, TT, US, VC, VG, VI" (IFCLABEL)
    RegionOceania (BO_oceania) = "AS, AU, CK, FJ, FM, GU, KI, MH, MP, NC, NF, NR, NU, NZ, PF, PG, PN, PW, SB, TK, TL, TO, TV, UM, WF, WS, VU" (IFCLABEL)
    RegionSouthAmerica (BO_southamerica) = "AR, BO, BR, CL, CO, EC, FK, GF, GY, PE, PY, SR, UY, VE" (IFCLABEL)
    SKU (BO_prodsku) = "hand_dryer_ibero_inox_220-240V_50-60hz" (IFCLABEL)
    TechnicalDescription (BO_techcert) = "https://jofel.com/media/fichas/en/AA92000.pdf" (IFCLABEL)
    UniFormat2Code (BO_uniformat2_code) = "" (IFCLABEL)
    UniFormat2Description (BO_uniformat2_name) = "" (IFCLABEL)
    Uniclass14Code (BO_uniclass_1_4_code) = "L824" (IFCLABEL)
    Uniclass14Description (BO_uniclass_1_4_desc) = "Bathroom, toilet furniture and fittings" (IFCLABEL)
    Uniclass2015Code (BO_uniclass2015_code) = "Pr_40_30_78_05" (IFCLABEL)
    Uniclass2015Description (BO_uniclass2015_desc) = "Bathroom furniture" (IFCLABEL)
    Uniclass20Code (BO_uniclass_2_0_code) = "PR-02-03" (IFCLABEL)
    Uniclass20Description (BO_uniclass_2_0_desc) = "Air Dryers" (IFCLABEL)
    UnspcCode (BO_unspc) = "301815" (IFCLABEL)
    Weight (BO_weight) = 3.655 (IFCREAL)
    Width (BO_width) = 280. (IFCREAL)